// Contents:   firmware to perform bulk loopback of EP2OUT to EP6IN and
//             EP4OUT to EP8IN using the PING NAK interrupt
//             to initiate the transfer.  Use with the cybulk host app.

