EzUsb FX2lp\eeprom images Directory:

The files in this directory include:

Fx2LP_C0.iic: the Default C0 load for FX2LP - identifies the Development Board platform.  This image can be programmed onto an FX2LP EEPROM using the EEPROM button on the EZ-USB Control Panel.

Fx2LP_C0.hex:  the Default C0 load for FX2LP - identifies the Development Board platform.  This image is in Intel Hex format and can be programmed onto an EEPROM using a standalone programmer.