FX1\eeprom images Directory:

The files in this directory include:

FX1_C0.iic: the Default C0 load for FX1 - identifies the Development Board platform.  This image can be programmed onto an FX2LP EEPROM using the EEPROM button on the EZ-USB Control Panel.

FX1_C0.hex:  the Default C0 load for FX1 - identifies the Development Board platform.  This image is in Intel Hex format and can be programmed onto an EEPROM using a standalone programmer.