hid_kb firmware
this firmware uses FX2LP or FX1 to emulate a USB HID keyboard.  On
the DVK board, buttons F1-F4 map to shift and a,b,c.  The
7-segment display shows the status of caps-lock, scroll-lock,
and num-lock.
